MANUAL 4-WAY SEAT ADJUSTER HANDLE INOPERATIVE. Chevrolet Corsica 1988

For 1990-2009 cars

# MANUAL 4-WAY SEAT ADJUSTER HANDLE INOPERATIVE

#### MODEL AND YEAR: 1988 BERETTA/CORSICA

Owners of some early production 1988 Beretta/Corsica Models may comment on the 4-way seat adjuster handle becoming disengaged from the seat adjuster assembly.

Should this condition occur DO NOT repair the adjuster assembly. REPLACE THE COMPLETE seat adjuster assembly with a new one.

Labor Operation Number: C6010 Right Side

C6011 Left Side

Labor Time : .3 Hour Remove and Replace

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.