Vehicle Speed Sensor and Governor Disassemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Using a socket wrench, remove the two bolts from the governor cover or from the speed sensor assembly (depending upon the application).
2. After you have removed the bolts (8), remove either the cover or the speed sensor assembly (802) (depending upon the application).
3. Remove the cover oil seal (7).
4. Remove the governor bearing (6).
5. Remove the governor assembly (4).
6. Remove the governor shaft oil seal (3).