Transmission Fluid Pan and Filter Assemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Install a new oil filter (33) into the case.
2. Clean the oil pan (35) and the magnet (38) in order to remove any sediment.
3. Inspect the oil pan for the following:

• | A damaged sealing surface

• | A dented or cracked bottom surface

4. Inspect the magnet (38) for damage.
5. Install a new oil pan gasket (38) onto the case.
6. Position the oil pan (35) onto the case.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

7. Finger start 16 bolts (36) into the pan and the case flange.

Tighten
Tighten the bolts to 11 N·m (98 lb in).