Evaporative Emission Canister Replacement. Chevrolet Corsica 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the left rear wheelhouse liner.
2. Remove the hoses from the canister. Mark the hoses to install on the new canister.
3. Loosen the latch on the canister bracket. Position out of the way.
4. Remove the canister from the vehicle.

### Installation Procedure

1. Install the canister to the vehicle.
2. Install the hoses to the canister as noted during removal.
3. Position the latch on the canister bracket.
4. Fasten securely.
5. Install the wheel house liner.