Valve Train Components Cleaning and Inspection. Chevrolet Corsica 1996

For 1990-2009 cars

Inspect the following areas:

• | Inspect the valve rocker arms and ball at the mating surfaces. These surfaces should be smooth and free of scoring or other damage.

• | Inspect the valve rocker arm valve pushrod sockets and valve stem mating surfaces. These surfaces should be smooth with no scoring or exceptional wear.

• | Inspect the valve pushrods for scored ends or bends.

• | Inspect the camshaft and crankshaft sprockets for wear

• | Timing chain for teeth that are no longer concentric

• | The valley between worn teeth

• | The key and crankshaft keyway for wear

• | The timing chain for binding or excessive wear