Torque Converter Clutch Solenoid and Wiring Harness Assemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Inspect the TCC solenoid (353) for damage or for cut wires.
2. Inspect the wiring harness assembly (339) for nicks, cuts, or damaged connectors.
3. Insert the TCC solenoid seal ring (337) onto the TCC solenoid (333).
4. Install the solenoid (333) into the auxiliary valve body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the bolt (334).

Tighten
Tighten the bolt to 11 N·m (98 lb in).

6. Connect the wire harness clip to the auxiliary control valve body.
7. On some models, connect the harness to the governor oil pressure switch.
8. On some models, connect the wire harness to the second clutch apply oil pressure switch.
9. Attach the wire harness (339) to the electrical connector.