SMU - SECTION 6E3 - DRIVEABILITY & EMISSIONS. Chevrolet Corsica 1995

For 1990-2009 cars

# SMU - SECTION 6E3 - DRIVEABILITY & EMISSIONS

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 6E3-DRIVEABILITY AND EMISSIONS REVISED CHART C-16A PCM CONTROLLED "LOW OIL LEVEL" LAMP

#### MODELS: 1994 CHEVROLET CORSICA, BERETTA WITH 2.3L ENGINE (VIN D - RPO LD2) 1994-1995 CHEVROLET CORSICA, BERETTA WITH 2.2L ENGINE (VIN 4 - RPO LN2)

THIS BULLETIN UPDATES CHART C-16A PCM CONTROLLED "LOW OIL LEVEL" LAMP, FOUND IN SECTION 6E3 ON PAGES C16-2, C16-3, IN THE 1994 SERVICE MANUAL AND PAGES C16-4, C16-5, IN THE 1994 AND 1995 SERVICE MANUAL.

FIGURES: 00 ATTACHMENTS: 02

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.