Fastener Tightening Specifications. Chevrolet Corsica 1996

For 1990-2009 cars

## Fastener Tightening Specifications Unit Repair

#### Fastener Tightening Specifications

Description of Usage | Qty | Size | Torque Assembly
--- | --- | --- | ---
Case cover to case | 4 | M8 x 1.25 x 45.0 | 24 N·m (18 lb ft)
Case cover to case | 4 | M8 x 1.25 x 55.0 | 24 N·m (18 lb ft)
Case cover to case | 1 | M8 x 1.25 x 40.0 | 24 N·m (18 lb ft)
Case cover to case | 7 | M8 x 1.25 x 25.0 | 24 N·m (18 lb ft)
Case cover to case | 2 | M8 x 1.25 x 25.0 | 24 N·m (18 lb ft)
Case to drive sprocket support | 4 | M8 x 1.25 x 23.5 | 24 N·m (18 lb ft)
Cooler connector | 2 | 1/4 - 18 NPSF | 38 N·m (23 lb ft)
Governor cover to case | 2 | M6 x 1.0 x 25.0 | 11 N·m (8 lb ft)
Intermediate servo cover | 4 | M6 x 1.0 x 20.0 | 11 N·m (8 lb ft)
Line pressure take-off | 1 | 1/8 - 27 NPTF | 11 N·m (8 lb ft)
Manual detent spring assembly to case | 1 | M6 x 1.0 x 10.0 | 11 N·m (8 lb ft)
Oil pan and valve body cover | 27 | M8 x 1.25 x 16.0 | 11 N·m (8 lb ft)
Parking lock bracket to case | 2 | M8 x 1.25 x 20.0 | 24 N·m (18 lb ft)
Pipe retainer to case | 2 | M8 x 1.25 x 14.0 | 24 N·m (18 lb ft)
Pressure switch (s) | 2 | 1/8 - 27 NPTF | 11 N·m (8 lb ft)
Pump cover to case cover | 1 | M8 x 1.25 x 130.0 | 24 N·m (18 lb ft)
Pump cover to valve body | 4 | M6 x 1.0 x 20.0 | 11 N·m (8 lb ft)
Pump cover to valve body | 3 | M6 x 1.0 x 90 | 11 N·m (8 lb ft)
Speedometer driven gear to governor cover | 1 | M6 x 1.0 x 16.0 | 9 N·m (75 lb in)
TCC Solenoid Valve to valve body | 1 | M6 x 1.0 x 16 | 11 N·m (8 lb ft)
TV cable to case | 1 | M6 x 1.0 x 16.0 | 9 N·m (75 lb in)
Valve body to case | 1 | M8 x 1.25 x 85.0 | 24 N·m (18 lb ft)
Valve body to case cover | 2 | M6 x 1.0 x 65.0 | 11 N·m (8 lb ft)
Valve body to case cover | 9 | M6 x 1.0 x 45 | 11 N·m (8 lb ft)
Valve body to driven sprocket support | 1 | M8 x 1.25 x 65.0 | 24 N·m (18 lb ft)