Flywheel to Torque Converter Bolt Replacement. Chevrolet Corsica 1996

For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Information.
2. Remove the transmission converter cover bolts.
3. Remove the transmission converter cover.
4. Mark the relationship of the converter to the flywheel.
5. Remove the three bolts that attach the converter to the flywheel.

### Installation Procedure

1. Install the bolts that attach the converter to the flywheel.

Tighten
Tighten all of the bolts to 62 N·m (46 lb ft). Re-torque the first bolt after all three have been tightened.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the converter cover.
3. Install the converter cover bolts.

Tighten
Tighten the converter cover bolts to 13 N·m (115 lb in).

4. Lower the vehicle.