UPDATE-MANUAL TRANSAXLE ON-CARSERVICING. Chevrolet Corsica 1990

For 1990-2009 cars

# UPDATE-MANUAL TRANSAXLE ON-CARSERVICING

#### Model and Year: 1990 L CAR (BERETTA GTZ) WITH 2.3L (VIN CODE A) ENGINE AND 5TM40 MANUAL TRANSMISSION

This bulletin supplements the procedure outlined in the 1990 Chevrolet L Car Service Manual on page 7B-14.

Prior to disconnecting the transaxle from the engine, the throttle body coolant pipes must be removed. The throttle body coolant pipes must never be bent to gain clearance. Removal of the throttle body coolant pipes is found in section 6B of the service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.