Automatic Transmission Range Selector Lever Replacement. Chevrolet Cruze (SGM) 2009

For 1990-2009 cars

### Removal Procedure

1. Set the park brake and chock the wheels.
2. Disconnect the transmission range selector lever cable terminal (1) from the transmission manual shift lever pin.
3. Press the locking tabs inward in order to release the transmission range selector lever cable (2) from the cable bracket.
4. Remove the transmission range selector lever fastener (1).
5. Remove the transmission range selector lever (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the transmission range selector lever (2).
2. Install the transmission range selector lever fastener (1).

Tighten
Tighten the fastener to 20 N·m (15 lb ft).

3. Install the transmission range selector lever cable (2) to the cable bracket.
4. Connect the transmission range selector lever cable terminal (1) to the transmission manual shift lever pin.
5. Check the range selector cable adjustment. Refer to Range Selector Lever Cable Adjustment.