Fuel Injection Pump Installation. Chevrolet Cruze (GME) 2010

For 1990-2009 cars

Caution:

• | Use care when servicing the fuel system components, especially the fuel injector electrical connectors, the fuel injector tips, and the injector O-rings. Plug the inlet and the outlet ports of the fuel rail in order to prevent contamination.

• | Do not use compressed air to clean the fuel rail assembly as this may damage the fuel rail components.

• | Do not immerse the fuel rail assembly in a solvent bath in order to prevent damage to the fuel rail assembly.

Note: Do not blow air with an air gun onto injection pump. If contaminated, wipe clean with an oilpaper.

1. Install the fuel pump (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 3 fuel pump bolts (2) and tighten to 30 N·m (23 lb ft).