Measuring Voltage Drop. Chevrolet Cruze (SGM) 2009

For 1990-2009 cars

Caution: Refer to Test Probe Caution in the Preface section.

The following procedure determines the difference in voltage potential between 2 points.

1. Set the rotary dial of the DMM to the V (DC) position.
2. Connect the positive lead of the DMM to one point of the circuit to be tested.
3. Connect the negative lead of the DMM to the other point of the circuit.
4. Operate the circuit.
5. The DMM displays the difference in voltage between the 2 points.