Battery Negative Cable Replacement. Chevrolet Cruze (SGM) 2009

For 1990-2009 cars

## Battery Negative Cable Replacement Gasoline

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the battery netative cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Battery Negative Cable Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)

2

Battery Negative Cable

#### Procedure

Transfer any parts as needed.