Front Bumper Fascia Extension Replacement. Chevrolet Cruze (SGM) 2009

For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1

Front Fascia Extension Screws (Qty: 5)

Caution: Refer to Fastener Caution in the Preface section.

Tip
The screws are located across the bottom of the fascia extension.

Tighten
2 N·m (18 lb in)

2 | Front Fascia Extension Tip Pull forward to release the fascia extension from the upper retainers.