CAMPAIGN:FRT. BRAKE PIPE AND ENGINE OIL PAN INTERFERENCE. Chevrolet El Camino 1980

For 1990-2009 cars

# CAMPAIGN:FRT. BRAKE PIPE AND ENGINE OIL PAN INTERFERENCE

THE NATIONAL TRAFFIC AND MOTOR VEHICLE SAFETY ACT, AS AMENDED, PROVIDES THAT EACH VEHICLE WHICH IS SUBJECT TO A RECALL CAMPAIGN OF THIS TYPE MUST BE ADEQUATELY REPAIRED WITHIN A REASONABLE TIME AFTER THE OWNER HAS TENDERED IT FOR REPAIR. A FAILURE TO ADEQUATELY REPAIR WITHIN 60 DAYS AFTER TENDER OF A VEHICLE IS PRIMA FACIE EVIDENCE OF FAILURE TO REPAIR WITHIN A REASONABLE TIME. IF THE CONDITION IS NOT ADEQUATELY REPAIRED WITHIN A REASONABLE TIME, THE OWNER MAY BE ENTITLED TO AN IDENTICAL OR REASONABLY EQUIVALENT VEHICLE AT NO CHARGE, OR TO A REFUND OF THE PURCHASE PRICE LESS A REASONABLE ALLOWANCE FOR DEPRECIATION.

IN ORDER TO AVOID HAVING TO PROVIDE THESE BURDENSOME SOLUTIONS, EVERY EFFORT MUST BE MADE TO PROMPTLY SCHEDULE AN APPOINTMENT WITH EACH OWNER AND TO REPAIR HIS VEHICLE AS SOON AS POSSIBLE. AS YOU WILL SEE IN READING THE ATTACHED COPY OF THE LETTER WHICH IS BEING SENT TO OWNERS, THE OWNER IS BEING INSTRUCTED TO CONTACT THE NEAREST CHEVROLET ZONE OFFICE IF HIS DEALER DOES NOT REMEDY THE CONDITION WITHIN FIVE DAYS OF THE MUTUALLY AGREED UPON SERVICE DATE. IF THE CONDITION IS NOT REMEDIED WITHIN A REASONABLE TIME HE IS INSTRUCTED ON HOW TO CONTACT THE NATIONAL HIGHWAY TRAFFICE SAFETY ADMINISTRATION.

DEFECT INVOLVED

SOME EARLY 1980 FULL SIZE CHEVROLETS EQUIPPED WITH LC3 229 CID, 3.8 LITRE V-6 ENGINES MAY HAVE INSUFFICIENT CLEARANCE BETWEEN THE FRONT BRAKE PIPE AND THE ENGINE OIL PAN. THIS CONDITION COULD CAUSE THE BRAKE PIPE TO COME IN CONTACT WITH THE LEFT HAND FRONT EDGE OF THE OIL PAN, RESULTING IN WEAR OF THE BRAKE PIPE AT THE POINT OF CONTACT.

PROLONGED CONTACT COULD CAUSE THE BRAKE PIPE TO WEAR THROUGH, RESULTING IN A LOSS OF BRAKE FLUID AND SUBSEQUENT LOSS OF FRONT BRAKES. THE DRIVER WOULD BE ALERTED TO BRAKE FLUID LOSS BY THE ILLUMINATION OF THE BRAKE WARNING LIGHT ON THE DASH PANEL AND BY AN INCREASE IN BRAKE PEDAL TRAVEL DURING BRAKE APPLICATION. THE REAR BRAKE SYSTEM WOULD REMAIN FUNCTIONAL. LOSS OF FRONT BRAKING AT A TIME WHEN MINIMUM STOPPING DISTANCE IS REQUIRED COULD RESULT IN VEHICLE CRASH WITHOUT PRIOR WARNING.

VEHICLES INVOLVED

INVOLVED ARE 1980 FULL SIZE CHEVROLETS EQUIPPED WITH LC3 229 CID, 3.8 LITRE V-6 ENGINES ASSEMBLED AT THE FOLLOWING GMAD ASSEMBLY PLANTS WITHIN THE FOLLOWING VEHICLE PARAMETERS:

PLANT FROM THROUGH

OSHAWA SOP 1N69KA1157998

JANESVILLE SOP 1N35HAJ212210

SOUTHGATE SOP 1N69KAC130622

ST. LOUIS SOP 1L47KAS121399

INVOLVED VEHICLES HAVE BEEN IDENTIFIED BY VEHICLE IDENTIFICATION NUMBER COMPUTER LISTINGS. COMPUTER LISTINGS CONTAIN THE COMPLETE VEHICLE IDENTIFICATION NUMBER, OWNER NAME AND ADDRESS DATA, AND ARE FURNISHED TO THE INVOLVED DEALERS WITH THE CAMPAIGN BULLETIN. OWNER NAME AND ADDRESS DATA FURNISHED WILL ENABLE DEALERS TO FOLLOW UP WITH OWNERS INVOLVED IN THIS CAMPAIGN.

THESE LISTINGS MAY CONTAIN OWNER NAME AND ADDRESSES OBTAINED FROM STATE MOTOR VEHICLE REGISTRATION RECORDS. THE USE OF SUCH MOTOR VEHICLE REGISTRATION DATA FOR ANY OTHER PURPOSE IS A VIOLATION OF LAW IN SEVERAL STATES. ACCORDINGLY, YOU ARE URGED TO LIMIT THE USE OF THIS LISTING TO THE FOLLOW-UP NECESSARY TO COMPLETE THIS CAMPAIGN. ANY DEALER NOT RECEIVING A COMPUTER LISTING WITH THE CAMPAIGN BULLETIN WAS NOT SHIPPED ANY INVOLVED VEHICLES.

OWNER NOTIFICATION

OWNERS WILL BE NOTIFIED OF THIS CAMPAIGN ON THEIR VEHICLES BY CHEVROLET MOTOR DIVISION (SEE COPY OF OWNER LETTER INCLUDED WITH THIS BULLETIN).

DEALER CAMPAIGN RESPONSIBILITY

DEALERS ARE TO SERVICE ALL VEHICLES SUBJECT TO THIS CAMPAIGN, REGARDLESS OF MILEAGE, AGE OF VEHICLE, OR OWNERSHIP, FROM THIS TIME FORWARD.

WHENEVER A VEHICLE SUBJECT TO THIS CAMPAIGN IS TAKEN INTO YOUR NEW OR USED VEHICLE INVENTORY OR IT IS IN YOUR DEALERSHIP FOR SERVICE IN THE FUTURE, YOU SHOULD TAKE THE STEPS NECESSRARY TO BE SURE THE CAMPAIGN CORRECTION HAS BEEN MADE.

PARTS INFORMATION

PARTS NECESSARY TO COMPLETE THIS CAMPAIGN MODIFICATION ARE TO BE FURNISHED FROM THE CHEVROLET ZONE SERVICE DEPARTMENT AND WILL BE FURNISHED ON A NO-CHARGE BASIS TO ALL INVOLVED DEALERS. THE PART WHEN REQUIRED TO COMPLETE THIS MODIFICATION IS IDENTIFIED AS FOLLOWS:

PART NUMBER QUANTITY DESCRIPTION

14031600 1 PER VEHICLE FRONT BRAKE PIPE

PARTS ARE NOT TO BE ORDERED OR RETURNED TO GENERAL MOTORS PARTS DIVISION.

SERVICE PROCEDURE

1. INSPECT THE BRAKE PIPE FOR CLEARANCE TO THE ENGINE OIL PAN. THERE SHOULD BE A MINIMUM OF 3/8" CLEARANCE AND IF THIS CLEARANCE IS PRESENT NO CORRECTIVE ACTION IS NEEDED.

2. IF THERE IS LESS THAN 3/8" CLEARANCE BETWEEN THE BRAKE PIPE AND THE ENGINE OIL PAN, BUT THE PIPE IS NOT IN CONTACT WITH THE PAN (AND THERE IS NO EVIDENCE THAT THERE HAS BEEN CONTACT) THEN REPOSITION THE PIPE FORWARD AND DOWNWARD TO OBTAIN THE PROPER CLEARANCES (3/8" TO ENGINE OIL PAN AND L/2" TO CROSSOVER PIPE). FINGER PRESSURE IS SUFFICIENT TO BEND THE PIPE - AVOID TOOLS THAT MAY DISTORT THE ROUNDNESS OF THE TUBE. CHECK TO SEE IF 3/8" CLEARANCE IS STILL PRESENT BETWEEN THE BRAKE PIPE AND BOTH RIGHT HAND AND LEFT HAND CORNERS OF THE ENGINE OIL PAN AFTER REPOSITION- ING PIPE.

3. IF THERE IS CONTACT BETWEEN THE BRAKE PIPE AND THE ENGINE OIL PAN, REPLACE THE BRAKE PIPE WITH BRAKE PIPE P/N 14031600 (1981 PRODUCTION PIPE). AFTER INSTALLING THE NEW PIPE, VERIFY THAT THE 3/8" CLEARANCE TO THE OIL PAN HAS BEEN MAINTAINED. FILL THE MASTER CYLINDER RESERVIOR WITH BRAKE FLUID, BLEED THE FRONT PIPE (RIGHT FRONT WHEEL) AND RE-CHECK THE FLUID LEVEL IN THE MASTER CYLINDER.

PART FAILED *PARTS FAILURE LABOR LABOR *OTHER COUNT PART NO. ALLOWANCE CODE OPERATION HOURS HOURS

00 V0581 .2 .1

DESCRIPTION: INSPECT BRAKE PIPE FOR PROPER CLEARANCE TO THE ENGINE OIL PAN ACCORDING TO THE INSTRUCTIONS OUTLINED IN THIS BULLETIN. NO FURTHER ACTION REQUIRED.

00 V0582 .2 .1

DESCRIPTION: INSPECT AND REPOSITION THE BRAKE PIPE IN ACCORDANCE WITH THE INSTRUCTIONS OUTLINED IN THIS BULLETIN.

1 14031600 .19 00 V0583 .6 .1

DESCRIPTION: INSPECT AND REPLACE THE BRAKE PIPE IN ACCORDANCE WITH THE INSTRUCTIONS CONTAINED IN THIS BULLETIN.

*CAMPAIGN ADMINISTRATIVE ALLOWANCE

** 30% OF DEALER NET ONLY FOR PARTS FURNISHED AT NO CHARGE BY CHEVROLET.

DEALERS WILL AUTOMATICALLY RECEIVE THE CORRECT PARTS AND LABOR ALLOWANCE BASED ON THE LABOR OPERATION PERFORMED. AMOUNTS ARE ENTERED ON CAMPAIGN CLAIMS TO ALLOW THE DEALER TO DEVELOP AN ACCOUNTS RECEIVABLE AMOUNT ONLY.

REFER TO THE CHEVROLET PROCESSING MANUAL FOR DETAILS ON PRODUCT CAMPAIGN CLAIM SUBMISSION.

CAMPAIGN IDENTIFICATION LABEL

EACH VEHICLE MODIFIED IN ACCORDANCE WITH THE INSTRUCTIONS OUTLINED IN THIS PRODUCT CAMPAIGN BULLETIN WILL REQUIRE A "CAMPAIGN IDENTIFICATION LABEL". EACH LABEL PROVIDES A SPACE TO INCLUDE THE FIVE DIGIT DEALER CODE OF THE DEALER PERFORMING THE CAMPAIGN SERVICE. THIS INFORMATION MAY BE INSERTED WITH A TYPEWRITER OR BALLPOINT PEN.

EACH "CAMPAIGN IDENTIFICATION LABEL" IS TO BE LOCATED ON THE RADIATOR CORE SUPPORT IN AN AREA WHICH WILL BE VISIBLE WHEN THE VEHICLE IS BROUGHT IN FOR PERIODIC SERVICING BY THE OWNER.

APPLY "CAMPAIGN IDENTIFICATION LABEL" ONLY ON A CLEAN DRY SURFACE.

ADMINISTRATIVE PROCEDURE

REFER TO THE CURRENT CHEVROLET SERVICE POLICIES AND PROCEDURES MANUAL AND CLAIMS PROCESSING MANUAL FOR CAMPAIGN HANDLING AND ADMINISTRATIVE PROCEDURES.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.