FRONT DOOR HINGE REPAIR CHECK LINK ROLLER. Chevrolet El Camino 1983

For 1990-2009 cars

# FRONT DOOR HINGE REPAIR CHECK LINK ROLLER

Front door hinges on Impalas, Caprices, Malibu and Monte Carlo with the check link roller may be repaired with P/N 20497383 (Figure 2) using the following procedure:

1. Using a #29 (.1360) drill bit, drill a hole 10mm (3/8") from the roller end of the hinge stop pin (Figure 1).

2. Thread drilled hole using a #8-32 tap.

3. Discard stop pin (Item 1, Figure 2) included in parts package.

4. Using a hammer, install roller, bushing and pin into hinge stop pin (Items 2, 3 and 4, Figure 2).

5. Install an 8-32 hexagon set screw (P/N 9426939 or equivalent) into tapped hole and tighten to retain roller pin. Apply Loctite thread sealer (P/N 1052624 or equivalent) to set screw threads prior to installation.

6. Install check link spring using tool J-29849 or equivalent.

7. Lubricate roller and bushing with 30 weight engine oil.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.