INTAKE MANIFOLD CHANGE 350 CID POLICE ENGINE. Chevrolet El Camino 1980

For 1990-2009 cars

# INTAKE MANIFOLD CHANGE 350 CID POLICE ENGINE

SHOULD A LOSS OF INTAKE GASKET SEALING BE ENCOUNTERED ON A 1980 OR 1981 POLICE VEHICLE EQUIPPED WITH 350 CID V-8 ENGINE AND ALUMINUM INTAKE MANIFOLD, A CAST IRON MANIFOLD (P/N 14031392) MAY BE INSTALLED. TWO (2) NEW HIGH TEMPERATURE (BLACK) INTAKE MANIFOLD SIDE GASKETS MUST BE INSTALLED WITH THE CAST IRON MANIFOLD. THE PROPER GASKETS ARE AVAILABLE IN KIT P/N 14038088 OR KIT P/N 14034821. THE INTAKE MANIFOLD BOLTS SHOULD BE TORQUED TO 30 FT. LBS. IN THE SPECIFIED SEQUENCE SHOWN IN FIGURE 6A 4-6 IN THE 1980 CHEVROLET SERVICE MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.