Front Side Door Window Replacement. Chevrolet Evaluator 1985

For 1990-2009 cars

### Removal Procedure

1. Position the front door window in the full down position.
2. Remove the front door trim panel.
3. Remove the front door water deflector.
4. Remove the outer belt sealing strip.
5. Remove the window weatherstrip.
6. Loosen the bolts (1) to the front and rear clevice clamps.
7. Remove the window from the outside of the front door.

### Installation Procedure

1. Position the window between the inner and the outer door panels.
2. Point the lower front corner of the window down and pass through the belt opening.
3. Align the edges with the window weatherstrip channel.

Notice: Refer to Fastener Notice in the Preface section.

4. Turn the window to a horizontal position and align the window with the front and rear clevice clamps.

Tighten
Tighten the front and rear clevice clamps bolts (1) to 11 N·m (97 lb in).

5. Install the window weatherstrip.

Important: Do not allow the sealing lips on the outer belt sealing strip to roll over and point downwards. If this condition is present the window will not raise properly.

6. Install the outer belt sealing strip.
7. Install the front door water deflector.
8. Install the front door inner trim panel.