Fastener Tightening Specifications. Chevrolet Evaluator 1985

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Auxiliary Weatherstrip Retainer Bolt | 2 N·m | 18 lb in
Door Arm Rest Screw | 3 N·m | 27 lb in
Door Glass Front Upstop-to-Door Glass Nut | 6 N·m | 53 lb in
Door Glass Rear Guide Retainer | 6 N·m | 53 lb in
Door Guide Pin Locator Screw | 11 N·m | 97 lb ft
Door Guide Pin Screw | 11 N·m | 97 lb ft
Door Hinge Bolt | 26 N·m | 19 lb ft
Door Hinge Nut | 26 N·m | 19 lb ft
Door Lock Screws | 10 N·m | 89 lb in
Door Rear View Mirror Nut | 6 N·m | 53 lb in
Door Sealing Strip Screw | 2 N·m | 18 lb in
Door Trim Panel Lower Screw | 2.5 N·m | 23 lb in
Door Trim Pull Cup Screw | 2.5 N·m | 23 lb in
Door Window Frame Applique Screw | 2 N·m | 20 lb in
Front and Rear Channel Adjustment Nutwasher | 10 N·m | 88 lb in
Front Channel-to-Door Stud Nuts | 6 N·m | 53 lb in
Front Door Upper Trim Finish Panel Screw | 1 N·m | 9 lb in
Lower Window Channel Bolt | 6 N·m | 53 lb in
Mirror Motor Retaining Screw | 10 N·m | 89 lb in
Mirror Set Screw | 1 N·m | 12 lb in
Rear Door Energy Absorber Bolt | 2 N·m | 18 lb in
Rear Door Lower Sealing Strip Screw | 2 N·m | 18 lb in
Rear Upper Extension-to-Door Nutwasher | 6 N·m | 53 lb in
Rear Upper Extension-to-Rear Channel Nutwasher | 6 N·m | 53 lb in
Rear Upstop Bracket Bolt | 6 N·m | 53 lb in
Regulator Bolts | 10 N·m | 89 lb in
Regulator Nuts | 10 N·m | 89 lb in
Reveal Molding Screw | 6 N·m | 53 lb in
Side Access Door Pull Handle Screw | 2.5 N·m | 23 lb in
Stabilizer Lock Nut | 6 N·m | 53 lb in
Stationary Window Channel Bolt | 10 N·m | 89 lb in
Striker Bolt | 25 N·m | 18 lb ft
Upper Window Channel Retainer Upper Bolt | 2 N·m | 18 lb in
Window Regulator-to-Door Screw | 6 N·m | 53 lb in
Window Sash Nuts | 10 N·m | 89 lb in