Frame, Actuator, Module, Track - Adjuster Driver Seat. Chevrolet Evaluator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications. Refer to Fastener Tightening Specifications (Link disabled for test). Drivers Front Seat. Refer to Seat Replacement - Front Bucket (Link disabled for test). Front Seat Cushion Cover and Pad. Refer to Seat Cushion Cover and Pad Replacement - Front (Link disabled for test).
1 | Nut, Driver Seat Frame Tighten: to 35 N·m (25 lb ft).
2 | Frame Assembly, Driver Seat
3 | Nut, Driver Seat Tilt Actuator Assembly Tighten: to 7 N·m (62 lb in).
4 | Actuator Assembly, Driver Seat Tilt Tip: Place the seat in the full up position to relieve tension on the motor. Remove the roll pin.
5 | Nut, Driver Seat Vertical Actuator Assembly Tighten: to 7 N·m (62 lb in).
6 | Actuator Assembly, Driver Seat Vertical Tip: Place the seat in the full up position to relieve tension on the motor. Remove the roll pin.
7 | Wiring Harness Assembly, Driver Seat Adjuster
8 | Screw, Driver Seat Horizontal Actuator Assembly (Qty:4) Tighten: to 3 N·m (26.5 lb in).
9 | Actuator Assembly, Driver Seat Horizontal Tip: Remove the adjuster motor cables by pulling the cables out of the adjuster.
10 | Retainer, Driver Seat Heater Control Module
11 | Module, Driver Seat Heater Control
12 | Track Assembly, Driver Seat Adjuster