Door Outside Handle Replacement. Chevrolet Evaluator 1985

For 1990-2009 cars

### Removal Procedure

1. Remove the cap to expose the T25 Torx head set bolt.
2. Remove the bolt (1).
3. Remove the outside cap (2).
4. Pull the outside handle (1) rearward and out of the door. Remove the outside handle.
5. Remove the gasket.
6. Remove the T25 Torx head bolt (1). Remove the handle housing.
7. Remove the door trim panel.
8. Remove the door water deflector.
9. Remove the lock rod (1) from the housing (2).
10. Remove the handle rod from the lock.

### Installation Procedure

1. Reverse the removal procedure.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the torx T25 bolt (1) to the handle housing.

Tighten
Tighten the bolt to 3 N·m (27 in lb)

3. Install the torx head cap. Install the T25 torx head bolt to the door frame side.

Tighten
Tighten the bolt to 3 N·m (27 in lb)