Tie Rod, Gear, Boot - Steering Gear. Chevrolet Evaluator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---

Fastener Tightening Specifications. Refer to Fastener Tightening Specifications .

Lift and suitably support the vehicle. Refer to Lifting and Jacking: in General Information. (Link disabled for test).

Remove the Wheel and Tire. Refer to Wheel and Tire Removal in Wheels and Tires. (Link disabled for test).

Front Toe Adjustment. Refer to Front Toe Adjustment in Wheel Alignment. (Link disabled for test).

1 | Nut, Steering Linkage Outer Tie Rod Tighten: to 60 N·m (44 lb ft)
2 | Nut, Steering Linkage Outer Tie Rod Jamb Tighten: to 60 N·m (44 lb ft)
3 | Rod, Steering Linkage Outer Tie Tip: Adjust the front toe angle after replacement. Tools Required: J 24319-B Tie Rod Separator
4 | Bolt, Intermediate Steering Shaft Tighten: to 49 N·m (36 lb ft)
5 | Shaft, Intermediate Steering Steering Column. Refer to Assembly - Steering Column in Power Steering. (Link disabled for test).
6 | Bolt, Steering Gear Tighten:1st Pass to 70 N·m (52 lb ft) 2nd Pass plus 90°
7 | Nut, Steering Gear Tighten1st Pass to 70 N·m (52 lb ft) 2nd Pass plus 90°
8 | Washer, Steering Gear
9 | Gear, Steering Tip: Rotate the steering gear 90 degrees and remove the gear from the left side of the vehicle.
10 | Clamp, Steering Gear Boot
11 | Clamp, Steering Gear Boot Tools Required: J 22610 Keystone Clamp Pliers
12 | Boot, Steering Gear