Hood, Hinge, Insulator, Rod, Latch, Cable - Body Front End. Chevrolet Evaluator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Notice .
1 | Bolt, Hinge Hood (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. TIP: Support the hood when replacing a hinge. Tighten 10 N·m (89 lb in)
2 | Hood Assembly TIP: Remove and install the hood with an assistant.
3 | Bolt, Hood Hinge Side (Qty: 4) Tighten 10 N·m (89 lb in)
4 | Hinge, Hood Side TIP: Support the hood when replacing a hinge.
5 | Retainer, Hood Insulator Push
6 | Insulator, Hood
7 | Retainer, Bumper Hood
8 | Bumper, Hood
9 | Bolt, Side Hinge (Qty: 4) TIP: Support the hood when replacing a hinge. Tighten 10 N·m (89 lb in)
10 | Rod Assembly, Hood Hold-Open
11 | Bolt, Primary Hood Release (Qty: 3) Tighten 10 N·m (89 lb in)
12 | Cable, Hood Primary Latch Release
13 | Latch, Hood Primary TIP: Inspect the latch before closing the hood.
14 | Bolt, Hood Hold --Open Rod Retainer (Qty: 1) Tighten 10 N·m (89 lb in)
15 | Retainer, Hood Hold --Open Rod