Antilock Brake System Schematic Icons. Chevrolet Evaluator 1985

For 1990-2009 cars

Icon | Icon Definition
--- | ---

Important: Twisted-pair wires provide an effective shield that helps protect sensitive electronic components from electrical interference. If the wires were covered with shielding, install new shielding.

In order to prevent electrical interference from degrading the performance of the connected components, you must maintain the proper specification when making any repairs to the twisted-pair wires shown :

• | The wires must be twisted a minimum of 9 turns per 31 cm (12 in) as measured anywhere along the length of the wires.

• | The outside diameter of the twisted wires must not exceed 6.0 mm (0.25 in).