Mirror, Cylinder, Handle, Door, Applique, Check Assembly, Hinge, Conduit - Outer Front Door. Chevrolet Evaluator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Fastener Notice .
1 | Housing Assembly, Outside Rear View Mirror
2 | Motor Assembly, Outside Rear View Mirror
3 | Mirror, Outside Rear View Mirror Replacement, refer to (Link Disabled For Test) in Body.
4 | Applique, Front Side Door Window Frame Rear
5 | Cylinder, Door Lock Door Handle Replacement, refer to Door Outside Handle Replacement , for additional detail.
6 | Handle Assembly, Front Side Door Outside
7 | Door Assembly, Front Side
8 | Molding, Door Body TIP: Ensure the temperature of the body and the body side molding is 29-32°C (85-90°F) for maxium flexibility.
9 | Bolts, Front Side Door Hinge Door Side Tighten: 26 N·m (19 lb. ft.)
10 | Hinge, Front Side Door Lower TIP: Minimize door realignment by replacing one hinge at a time.
11 | Bolts, Front Side Door Hinge Door Side Tighten: 26 N·m (19 lb. ft.)
12 | Conduit, Front Side Door Wiring
13 | Nut, Front Side Door Check Tighten: 26 N·m (19 lb. ft.)
14 | Check Assembly, Front Door
15 | Bolt, Front Side Door Check Link Tighten: 26 N·m (19 lb. ft.)
16 | Bolts, Front Side Door Hinge Body Side Tighten: 26 N·m (19 lb. ft.)
17 | Bolt, Front Side Door Hinge Tighten: 26 N·m (19 lb. ft.)
18 | Hinge, Front Side Door Upper TIP: Minimize door realignment by replacing one hinge at a time.