3rd and 4th Clutch Accumulator Housing Removal. Chevrolet Export Express 2000

For 1990-2009 cars

1. Remove the 3rd and 4th clutch accumulator housing bolts (53).
2. Remove the 3rd and 4th clutch accumulator housing (51).
3. Remove the accumulator housing gasket (47). The accumulator housing gasket (47) may be stuck to the control valve body spacer plate (46).
4. Remove the 3rd clutch accumulator piston spring (50).
5. Remove the 4th clutch accumulator piston spring (49).
6. Remove the control valve body spacer plate (46).
7. Remove the control valve body gasket (45) from the control valve body spacer plate (46).