Direct Clutch Assembly Installation. Chevrolet Export Chevy P32 RV/VAN Chassis 1999

For 1990-2009 cars

#### Tools Required

• | J 24396 Intermediate Clutch Pack Alignment Tool

• | J 38733 Direct Clutch Assembly Remover/Installer

1. Using the J 24396 , align the intermediate clutch plates.
2. Apply compressed air through the center support bolt hole to apply the intermediate clutch. Continue applying compressed air to hold the intermediate clutch plates in place until the direct clutch assembly is installed.
3. Remove the J 24396 .
4. Using the J 38733 , install the direct clutch housing assembly (623) into the transmission case. Rotate the direct clutch housing assembly slightly in each direction to ease installation.
5. Remove the J 38733 .