Forward Clutch Assembly Installation. Chevrolet Export Express 1999

For 1990-2009 cars

#### Tools Required

• | J 36850 Transjel® Lubricant

• | J 38358-A Forward Clutch Assembly Remover/Installer

1. Align the direct clutch plates in order to aid in the installation of the forward clutch housing assembly (602).

Important: Following installation of the forward clutch housing assembly (602), the distance between the top of the speed sensor ring and the pump gasket surface should be approximately 98-99 mm (3.85-3.89 in).

2. Using the J 38358-A , install the forward clutch housing assembly (602).
3. Install the overdrive carrier/forward clutch thrust bearing assembly (601) (silver side up) onto the forward clutch housing assembly (602). Retain with J 36850 or equivalent.