Hood Hold-Open Rod Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Hood Hold-Open Device Caution in the Preface section.

1. Support the hood in the open position.
2. Using a sharp gimlet, press the pins (2).
3. Remove the hood prop (1) from the hood.
4. Remove the hood prop rod (1) from the hood prop.

### Installation Procedure

1. Install the hood prop rod to the hood prop.
2. Install the hood prop to the hood with the pins.