Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Blower Module Nuts | 3-5 N·m | 27-44 lb in
Heater Module Nuts | 3-5 N·m | 27-44 lb in
Compressor-to-Bracket Upper Bolt | 20 N·m | 15 lb ft
Compressor-to-Bracket Lower Bolt | 22 N·m | 16 lb ft
High Pressure Pipe Line Bolt | 23 N·m | 17 lb ft
Low Pressure Pipe Line Bolt | 23 N·m | 17 lb ft
Shaft Bolt | 13 N·m | 115 lb in
High Pressure Pipe Line to Condenser Pipe Line Fitting | 23 N·m | 17 lb ft
High Pressure Pipe Line to Receiver Dryer Fitting | 14 N·m | 10.5 lb ft
High Pressure Pipe Line Bracket Nut | 5 N·m | 44 lb in
Receiver Dryer Flange Nuts | 14 N·m | 10.5 lb ft
High Pressure Pipe Line to Evaporator Nut | 14 N·m | 10.5 lb ft
High Pressure Pipe Line Bracket Nut | 5 N·m | 44 lb in
Low Pressure Pipe Line to Evaporator Nut | 14 N·m | 10.5 lb ft
Bracket Nut | 5 N·m | 44 lb in
Low Pressure Pipe Line to Compressor Bolt | 23 N·m | 17 lb ft
High Pressure Pipe Line Nut | 14 N·m | 10.5 lb ft
Low Pressure Pipe Line Nut | 14 N·m | 10.5 lb ft
Expansion Valve Fitting | 22 N·m | 16 lb ft
High Pressure Line Fitting | 17 N·m | 13 lb ft
Dual Cut Switch | 13 N·m | 115 lb in
Dual Cut Switch Bracket Bolt | 5 N·m | 44 lb in
Receiver Dryer Flange Nut | 14 N·m | 10.5 lb ft
Receiver Dryer Bracket-to-Body Bolt | 5 N·m | 44 lb in
Receiver Dryer Bracket Bolt | 5 N·m | 44 lb in
Condenser Mounting Nuts | 4 N·m | 36 lb in
Condenser Pipe to Compressor Pipe Fitting | 23 N·m | 17 lb ft
Condenser Pipe to Receiver Dryer Pipe Fitting | 14 N·m | 10.5 lb ft