Windshield Wiper Transmission Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the windshield wiper arms. Refer to Windshield Wiper Arm Replacement .
2. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
3. Separate the wiper linkage (1) from the wiper motor.
4. Remove the wiper linkage nuts (2).
5. Remove the wiper linkage (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the wiper linkage with the wiper linkage nuts (1).

Tighten
Tighten the wiper linkage nuts to 1.5-2 N·m (13-18 lb in).

2. Install the wiper motor linkage ball.
3. Install the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
4. Install the windshield wiper arms. Refer to Windshield Wiper Arm Replacement .