Engine Coolant Fan Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Caution: Refer to Electric Coolant Fan Caution in the Preface section.

Caution: Refer to Damaged Fan Blade Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the cooling fan electrical connector (3).
3. Remove the bolts (2).
4. Remove the electric cooling fan assembly (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the electric cooling fan assembly with the bolts (1).

Tighten
Tighten the bolts to 3.5-4.5 N·m (31-40 lb in).

2. Connect the cooling fan electrical connector.
3. Connect the negative battery cable.