Instrument Panel Inflatable Restraint Module Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling .
2. Remove the glove box. Refer to Instrument Panel Storage Compartment Replacement .
3. Remove the center instrument panel bezel. Refer to Instrument Panel Outer Trim Cover Replacement .
4. Disconnect the I/P module connector (1).
5. Remove the 2 I/P module fasteners (1).
6. Remove the 4 I/P module fasteners (1).
7. Remove the 2 I/P module fasteners (2).
8. Remove the I/P module.

### Installation Procedure

1. Install the I/P module.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 2 I/P module fasteners (2).

Tighten
Tighten the 2 I/P module fasteners (2) to 12 N·m (106 lb in).

3. Install the 4 I/P module fasteners (1).

Tighten
Tighten the 4 I/P module fasteners (1) to 10 N·m (89 lb in).

4. Install the 2 I/P module fasteners (1).
5. Connect the I/P module connector (1).
6. Install the center instrument panel bezel. Refer to Instrument Panel Outer Trim Cover Replacement .
7. Install the glove box. Refer to Instrument Panel Storage Compartment Replacement .
8. Enable the SIR system. Refer to SIR Disabling and Enabling .