Suspension Component Inspection. Chevrolet Joy 2008

For 1990-2009 cars

Table 1: | Noise
Table 2: | Uncomfortable
Table 3: | Vehicle Leans Toward the Side

#### Noise

Checks | Actions
--- | ---
Loose joints | Tighten the joints.
Worn or damaged wheel bearing | Replace the wheel bearing.
Faulty shock absorber | Replace the shock absorber.

#### Uncomfortable

Checks | Actions
--- | ---
Faulty shock absorber | Replace the shock absorber.
Faulty coil spring | Replace the coil spring.
Trailing arm bushing is worn or damaged | Replace the trailing arm bushing.

#### Vehicle Leans Toward the Side

Checks | Actions
--- | ---
Rear axle deformation | Replace the rear axle.
Trailing arm deformation | Replace the rear axle.
Faulty coil spring | Replace the coil spring.
Trailing arm bushing is worn or damaged | Replace the trailing arm bushing.