Evaporative Emission Canister Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Fuel and Evaporative Emission Pipe Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

Caution: Fuel Vapors can collect while servicing fuel system parts in enclosed areas such as a trunk. To reduce the risk of fire and increased exposure to vapors:

• | Use forced air ventilation such as a fan set outside of the trunk.

• | Plug or cap any fuel system openings in order to reduce fuel vapor formation.

• | Clean up any spilled fuel immediately.

• | Avoid sparks and any source of ignition.

• | Use signs to alert others in the work area that fuel system work is in process.

1. Disconnect the negative battery cable.
2. Remove the canister bolt (1).
3. Remove the canister nut and the cover (2).
4. Disconnect the canister hoses (2).
5. Remove the evaporative emission canister (1).

### Installation Procedure

1. Install the evaporative emission canister (1).
2. Connect the canister hoses (2).
3. Install the canister cover (2), bolt (1) and nut.
4. Connect negative battery cable.