Front Seat Cushion Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front seat assembly. Refer to Front Seat Replacement - Bucket .
3. Remove the seat belt buckle. Refer to Front Seat Belt Buckle Replacement .
4. Remove the recliner knob screw (2).
5. Remove the recliner knob (1).
6. Remove the recliner cover screws (2).
7. Remove the recliner cover (1).
8. Remove the recliner bolts on the seat cushion (3).
9. Remove the seat back bolt (2).
10. Remove the seat cushion (1).

### Installation Procedure

1. Install the seat cushion with the seat back bolt and the recliner bolts.
2. Install the recliner cover and the recliner knob with the screws.
3. Install the seat belt buckle. Refer to Front Seat Belt Buckle Replacement .
4. Install the front seat assembly. Refer to Front Seat Replacement - Bucket .
5. Connect the negative battery cable.