Fender Liner Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front wheels. Refer to Tire and Wheel Removal and Installation .
3. Remove the clip and bolts.
4. Remove the front fender liner.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Remove the front fender liner.
2. Install the clip and bolts.
3. Install the front wheels. Refer to Tire and Wheel Removal and Installation .
4. Lower the vehicle.