Park/Neutral Position Switch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Replacement Procedure

#### Tools Required

• | DT 47529 (DW 260-240) - Spring Pin Remover

• | DT 47530 (DW 260-250) - Spring Pin Installer

1. Remove the gearshift control cable. Refer to Shift Cable Replacement .
2. With DT 47529 (1), remove the spring pin (3) and the select lever assembly (2).
3. Remove the bolt and the shift lever switch (1).

### Adjustment Procedure

1. Position the select lever assembly to "N".
2. Loosen the shift switch fixing bolt.
3. Fix the select lever assembly inserting a 3 mm (0.12 in) pin (drill) (1) into the location holes of the assembly and the shift switch.
4. Tighten the shift switch bolt.

Tighten
Tighten the bolts of the shift lever switch to 3 N·m (26 lb in.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the shift lever switch through the manual shaft, and temporarily tighten the bolt.
2. Embed the select lever assembly in the manual shaft, and punch the spring pin using the DT 47530 (1).
3. Move the select lever assembly to shift into the "N" range.
4. Insert a 3 mm (0.12 in) pin (drill) (1) in the location holes of the shift lever switch and the select lever assembly.

Tighten
Tighten the bolts of the shift lever switch to 3 N·m (26 lb in).

5. Install the gear shift control cable. Refer to Shift Cable Replacement .