Seat Belt Replacement - Center Rear. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion.
2. Remove the 2-point seat belt and the 3-point buckle by removing the bolt and the fiber washer (1).
3. Remove the 2-point and 3-point buckles by removing the bolt and the fiber washer (3).

### Installation Procedure

Caution: Refer to Seat Belt Replacement Caution in the Preface section.

Notice: Refer to Fastener Notice in the Preface section.

1. Install the 2-point and 3-point buckles with the bolt (2) and the fiber washer.

Tighten
Tighten the 2-point and 3-point rear seat belt buckle bolt to 30-45 N·m (22-33 lb ft).

2. Install the 2-point seat belt and the 3-point buckle with the bolt (1) and the fiber washer.

Tighten
Tighten the 2-point rear seat belt bolt and 3-point rear seat belt buckle bolt to 30-45 N·m (22-33 lb ft).

3. Install the rear seat cushion.