Engine Cooling System Specifications. Chevrolet Joy 2008

For 1990-2009 cars

## Engine Cooling System Specifications 0.8L

Application | Specification
--- | ---
Metric | English
Cooling System

- Cooling Type

Forced Water Circulation

Coolant

- Coolant Capacity

4.2 L

4.44 qt

Thermostat

- Thermostat Type

Pellet Type

- Temperature (Opened Initially)

82°C

180°F

- Temperature (Perfectly Opened)

95°C

203.4°F

- Temperature (Perfectly Closed)

80°C

176.4°F

- Stroke (perfectly opened)

8 mm

0.32 in

Electric Cooling Fan

- Cooling Fan Type

Electric

- Blade Number

6

- Cooling Fan Diameter

300 mm

11.8 in

- Temperature at Low Speed ON

93°C

199.8°F

- Temperature at Low Speed OFF

90°C

194.4°F

- Temperature at High Speed ON

100°C

212.4°F

- Temperature at High Speed OFF

95°C

203°F

Surge Tank

- Open Pressure of the Pressure Valve

120-160 kPa

17.4-23.2psi

- Open Pressure of the Vacuum Valve

10 kPa

1.5 psi

Coolant Pump

- Water Pump Type

Centrifugal

- Impeller Diameter

60 mm

2.36 in

- Impeller Blade Number

7 EA

Radiator

- Radiator Type

Cross-Flow

- Core Width

458 mm

18.03 in

- Core Height

295 mm

11.61 in

- Core Depth (Standard/Heavy Duty)

16/27 mm

0.63/1.06 in

Coolant Temperature Sensor

- Resistance (Coolant Temperature 50°C (122.4°F))

185.2 ohms

- Resistance (Coolant Temperature 85°C (185.4°F))

49.2 ohms

- Resistance (Coolant Temperature 105°C (221.4°F))

27.5 ohms

- Engine Coolant Temperature SensorResistance (Coolant Temperature 20°C (68.4°F))

3,520 ohms

- Engine Coolant Temperature SensorResistance (Coolant Temperature 80°C (176.4°F))

332 ohms