Rear Wheel Bearing and Hub Replacement. Chevrolet Joy 2008

For 1990-2009 cars

#### Tools Required

• | J 8092 Universal Driver Handle - 3/4 in. - 10

• | CH 46566 Rear Wheel Bearing Race Installer

### Disassembly Procedure

1. Remove the rear brake drum. Refer to Brake Drum Replacement .
2. Remove the outer tapered roller bearing (1).
3. Remove the oil seal (1).
4. Remove the inner tapered roller bearing (2).
5. Remove the inner bearing race from the brake drum (1).
6. Remove the outer bearing race from the brake drum (1).

### Assembly Procedure

Important: Use a new bearing.

1. Press the inner bearing race into the brake drum using J 8092 (1) and CH 46566 (3).
2. Press the outer bearing race into the brake drum using J 8092 (1) and CH 46566 (3).
3. Apply wheel bearing lubricant to the wheel bearing and to the ring seal lip.
4. Install the inner wheel bearing (2) into the brake drum.
5. Install the oil seal (1) into the brake drum.
6. Install the outer wheel bearing (1) into the brake drum.
7. Install the brake drum. Refer to Brake Drum Replacement .
8. Inspect the end play and free load of the bearing. Refer to Bearings Inspection .
9. Lower the vehicle.