Front Fender Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the fender liner. Refer to Fender Liner Replacement .
3. Remove the fender mounting lower bolt (2) at the base of the fender.
4. Open the front door. Remove the fender mounting bolt (1) on the windshield pillar.
5. Remove the bumper fascia side bolts (1) on the side of the front bumper fascia.
6. Remove the fender mounting bolt (2) under the fender.
7. Lower the vehicle.
8. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
9. Remove the mounting bolts on top of the fender.
10. Remove the bolts along the top of the fender.
11. Remove the fender.

### Installation Procedure

1. Install the fender and align.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts along the top of the fender.

Tighten
Tighten the top fender bolts to 10 N·m (89 lb ft).

3. Install the upper fender mounting bolts.

Tighten
Tighten the upper fender mounting bolts to 10 N·m (89 lb ft).

4. Install the air inlet grille. Refer to Air Inlet Grille Panel Replacement .

Caution: Refer to Vehicle Lifting Caution in the Preface section.

5. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
6. Install the bolt (2) under the fender.

Tighten
Tighten the fender bolt to 10 N·m (89 lb ft).

7. Install the bolts (1) on the side of the front bumper fascia.

Tighten
Tighten the front bumper fascia bolts to 1.5 N·m (13 lb in).

8. Open the front door and install the bolt (1) on the windshield pillar.

Tighten
Tighten the fender bolt to 10 N·m (89 lb ft).

9. Install the bolt (2) at the base of the fender.

Tighten
Tighten the fender bolt to 10 N·m (89 lb ft).

10. Install the fender liner. Refer to Fender Liner Replacement .
11. Lower the vehicle.