Front Seat Replacement - Bucket. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front seat bolts (2).
3. Disconnect the seat belt warning lamp connector (3).
4. Remove the front seat (1).

### Installation Procedure

1. Connect the seat belt warning lamp connector

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front seat with the bolts (1).

Tighten
Tighten the seat bolt to 35 N·m (26 lb ft).

3. Connect the negative battery cable.