Headlamp Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Support the hood suitably.

Caution: Refer to Battery Disconnect Caution in the Preface section.

2. Remove the headlamp bolts and washer.
3. Disconnect the electrical connectors.
4. Remove the headlamp.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the headlamp with the bolts.

Tighten
Tighten the bolts to 4 N·m (35 lb in).

2. Connect the headlamp electrical connectors.
3. Connect the negative battery cable.