Radio Display Inoperative, No Sound from Speakers. Chevrolet Joy 2008

For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Radio/Navigation System Schematics
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Verify the fault is present. Does the system operate normally? | -- | System OK | Go to Step 3
3 | Check fuses F18 and F3. Are fuses F18 and F3 blown? | -- | Go to Step 4 | Go to Step 5

4

1. Check for a short circuit and repair it, if necessary.
2. Replace the blown fuses.

Is the repair complete?

--

Go to Step 12

--

5

1. Use a voltmeter to test for battery voltage at fuse F18.
2. Turn the ignition ON and test for battery voltage at fuse F3.

Does the battery voltage match the specified value at fuses F18 and F3?

11-14V

Go to Step 7

Go to Step 6

6 | Repair the power supply circuit to the fuses. Is the repair complete? | -- | Go to Step 12 | --

7

1. Remove the cassette radio.
2. Turn the ignition ON.
3. Use a voltmeter to test for battery voltage at the audio system connector terminals 15 and 8.

Does the battery voltage match the specified value at both terminals?

11-14V

Go to Step 9

Go to Step 8

8 | Repair the open circuit between the audio system connector and the fuse. Is the repair complete? | -- | Go to Step 12 | --
9 | Use an ohmmeter to test the ground circuit at the audio system connector terminal 16. Does the resistance match the specified value? | 0 ohms | Go to Step 11 | Go to Step 10
10 | Repair the open ground circuit between the audio system connector and ground G202. Is the repair complete? | -- | Go to Step 12 | --
11 | Replace the cassette radio. Is the repair complete? | -- | Go to Step 12 | --
12 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 1