Rear Wiper Always On. Chevrolet Joy 2008

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Wiper/Washer Schematics Connector End View Reference: Wiper/Washer Connector End Views DEFINITION: This table diagnoses the rear wipers are always on when the rear wiper/washer switch is in the OFF position.
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle

2

1. Turn the ignition ON, engine OFF.
2. Verify that the rear wipers are always ON when the wiper/washer switch is in the OFF position.

Are the rear wipers always ON?

Go to Step 3

Go to Testing for Intermittent Conditions and Poor Connections

3

1. Turn the ignition OFF.
2. Disconnect the wiper/washer switch.
3. Turn the ignition ON, engine OFF.

Are the rear wipers always ON?

Go to Step 5

Go to Step 4

4 | Replace the rear wiper/washer switch. Did you complete the replacement? | Go to Step 6 | --
5 | Repair the short to voltage condition. Refer to Wiring Repairs . Did you complete the repair? | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | --