Exhaust Manifold Removal. Chevrolet Joy 2008

For 1990-2009 cars

Caution: Refer to Exhaust Service Caution in the Preface section.

1. Remove the air filter resonator, and snorkel assembly. Refer to Air Cleaner Assembly Replacement for the 1.0L engine.
2. Disconnect the ignition wire and oxygen sensor (O2S) connector.
3. Remove exhaust manifold heat shield.
4. Remove the exhaust pipe from the pup-up catalytic converter .
5. Remove the exhaust manifold with pup-up catalytic converter.
6. Remove the exhaust manifold from pup-up catalytic converter.