Door Lock Cylinder Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the outside door handle. Refer to Front Side Door Outside Handle Replacement .
3. Remove the clip (2).
4. Remove the door lock cylinder (1) from the outside door handle.

### Installation Procedure

1. Install the door lock cylinder (1) with the clip (2) to the outside door handle.
2. Install the outside door handle. Refer to Front Side Door Outside Handle Replacement .
3. Connect the negative battery cable.