Shock Absorber Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Support the rear axle (1) with adjustable jack stands.
3. Remove the nuts (1, 3).
4. Remove the shock absorber (2).

### Installation Procedure

1. Install the shock absorber (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nut (3) which secures the shock absorber to the rear axle.

Tighten
Tighten the nut to 58 N·m (42 lb ft).

3. Install the nut (1) which secures the shock absorber to the body bracket.

Tighten
Tighten the nut to 58 N·m (42 lb ft).

4. Remove the jack stands.
5. Lower the vehicle.